Please follow the Steps below to upgrade your device:

1. Please download the firmare file to your PC and unzip it;
2. Copy the firmware file (FW96650A.bin) to a formatted microSD card and plug the card to the dash cam;

***Note:*** *the firmware file (in .bin format) could not be recognized by computer, it could just be recognized by the dash cam, so don’t try to open it on PC, just copy it to the card.*

1. Plug the camera to a power charger (not computer), or press the power button;
2. Then the camera will auto upgrade, and it will take about 30 secs to 1 min, during this time, the camera will not turn on and will not respond to any button or operation;
3. Once the dash cam upgraded successfully, it will turn on and work.
4. Please have a check the version of your device now (go to the System Setup menu and turn to the Version) and see if it is VTN16H.V1. If it is, then the camera has been upgraded successfully.
5. Format your microSD card on the camera again when the update has been completed, or the camera will upgrade itself everytime when it detects the firmware file in the card.

Thank you!

Any question, please contact us at [support@vantrue.net](mailto:support@vantrue.net).

Best regards,

Vantrue Team